**Hirox Digital Microscope KH-7700, Lens MX – 2016Z, Adapter AD – 2016S.**

Measure > Calibration > Select from MAG LENS LIST

[Put asterix on left side onto correct lens] APPLY, CLOSE.

Measure > 2D MEASUREMENT

 Linear measurement (Do not check ‘RATIO’)

Length = click once and measure LONGEST axis and click end.

Width = repeat for shorter axis.

**To delete a measurement use the Dustbin button.**

**AREA**

**Check area box only.**

Click repeatedly around object perimeter and double click to finish.

**SAVE MEASUREMENTS (µm are appropriate)**

Files are .csv format

Blue cross button to close measurements.

LIBRARY>LIBRARY>to copy files to USB or CD.